# SDR receiver compatible with HPSDR

The Red Pitaya SDR receiver is ready.

Now you can run the SDR programs that support the HPSDR/Metis protocol.

More details about this application can be found at this link.

### SDR programs

Here is a list of the SDR programs that are known to work with this SDR receiver:

- PowerSDR mRX PS that can be downloaded from this link
- QUISK with the hermes/quisk_conf.py configuration file
- CW Skimmer Server and RTTY Skimmer Server
- ghpsdr3-alex client-server distributed system
- openHPSDR Android Application that is described in more details at this link
- Java desktop application based on openHPSDR Android Application

### Running CW Skimmer Server

- Install CW Skimmer Server.
- Copy HermesIntf.dll to the CW Skimmer Server program directory (C:\Program Files (x86)\Afreet\SkimSrv).
- Install Reverse Beacon Network Aggregator.
- Start CW Skimmer Server, configure frequencies and your call sign.
- Start Reverse Beacon Network Aggregator.