Calibrating...
0 kB/s

#### Export

Content

#### Settings

Content settings
Measuring...
Current step: 1Current freq: 1Hz
Amplitude [dB]
Phase [deg]
Frequency [Hz]

#### Calibration

To calibrate your setup connect IN2 to IN1 (bypass DUT) and press CALIBRATE.

#### Licence missing

Application is running in demo mode!

Please visit Red Pitaya store to get the licence.

#### Oops, something went wrong

Please send us the report and help us to fix this issue

Thank you!

#### Diagnostic & Usage

Would you like to help Red Pitaya team to improve its product and services by occasionally providing anonymous diagnostic and usage information?

FPS:0 Throughput:0 CPU Load:0
Memory total:0 Free:0 Usage:0
Performance problem has occurred
You are working in demo mode. Click here to see details.