P. DISP: Z
S. DISP: P
MODE: AUTO
FREQ.: 100Hz
MIN: -
MAX: -
AVG: -
0 --
0 --

# | Z | P
--- | --- | ---

#### Starting calibration process...

10% Complete

##### Please connect open calibration circuit and press start

#### Calibrating....

50%

##### Please connect short calibration and press next

#### Calibrating.....

100%

##### You have successfully calibrated your Red Pitaya.

#### Unable to load application.

##### E3: Socket not opened. Press Reload to reload the application.

#### Time-out.

##### Socket closed. Press reload to reload the application.

#### Extension module status

##### Extension module is not connected

#### Extension module status

##### I2C-tool not installed

#### Licence missing

Application is running in demo mode!

Please visit Red Pitaya store to get the licence.

#### Oops, something went wrong

Please send us the report and help us to fix this issue

Thank you!

#### Diagnostic & Usage

Would you like to help Red Pitaya team to improve its product and services by occasionally providing anonymous diagnostic and usage information?

You are working in demo mode. Click here to see details.