SCPI server application

- enables remote control of Red Pitaya using MATLAB/Python/LabVIEW/Scilab
- provides comlete access to Red Pitaya hardware functionalities
  (GPIO, slow and fast DACs and ADCs, I2C, SPI, UART)
- supports WIFI or LAN remote interface

SCPI server is not running, press RUN button to start it
SCPI server is running... (IP="127.0.0.1", port="5000")

- RUN
- STOP

Click here to see the example about how to Control your Red Pitaya using MATLAB/Python/LabVIEW/Scilab.
FPS:0 Throughput:0 CPU Load:0
Memory total:0 Free:0 Usage:0

#### Oops, something went wrong

Please send us the report and help us to fix this issue

Thank you!

#### Diagnostic & Usage

Would you like to help Red Pitaya team to improve its product and services by occasionally providing anonymous diagnostic and usage information?